ESI U2A Driver Update for Windows 98/ME/2000/XP
16-DEC-2004
Copyright 2004 ESI
All Rights Reserved

======================================================================

This file contains additions and changes to the printed manual. Please
read this information before installing U2A update.

======================================================================
INSTALLATION
======================================================================

This updated U2A driver has two parts.

Part 1 - USB ASIO Driver Installation.
1. To start installation, run SetupXP2k.exe for 2000/XP, or run Setup98ME.exe for 98/ME.
2. Read & follow steps in Install.pdf file.

Part 2 - U2A Control Panel.
1. Copy U2A.exe to your desired location and run it when needed.

Thanks for choosing ESI.

Audiotrak

                   < END OF FILE >